**Technical data DRYVAC DV 200**

|  |  |
| --- | --- |
| Max. pumping speed | 210 m3/h124 cfm |
| Ultimate pressure (w/o gas ballast) | < 0.05 mbar< 0.04 Torr |
| Permissible ambient temperature | 5 to 50 °C |
| Noise level with silencerat ultimate pressure | 65 dB(A) |
| Relative ambient atmospheric humidity | 90%, non-condensing |
| Max. installation height | Up to 2000 m above sea level |
| Cooling | Water |
| Cooling water temperature range | 5 to 35 °C |
| Cooling water nominal flow | 8 l/min |
| Mains voltage 50/60 Hz | 200-240 V ±10% or380-460 V ±10% |
| Rated power 50/60 Hz | 7.5 kW |
| Power consumption at ultimate pressure | 4.1 kW |
| Bearing lubricant | LVO 210 synthetic oil |
| Protection class | IP54 |
| Intake connection | DN 63 ISO-K |
| Discharge flange | DN 40 ISO-KF |
| Weight, approx. | 370 kg |
| Dimensions (W x H x D) | 1110 mm x 613 mm x 478 mm |